<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">CMOSMap 1.8.1, BA, 26, 26, BIOS, 1bh, d1h, Port72

CompressedSetupDataSegment 4f14h
MainMenu 4728h
CMOSName CMOS_KbdRequired, reboot, 01bh, 002h, 001h, 000h
CMOSName CMOS_CRTRequired, reboot, 01bh, 006h, 001h, 000h
CMOSName CMOS_NumLock, reboot, 01bh, 007h, 001h, 001h
CMOSName CMOS_AlternateBootDevice4, reboot, 01dh, 000h, 004h, 008h
CMOSName CMOS_AlternateBootDevice3, reboot, 01dh, 004h, 004h, 00ch
CMOSName CMOS_AlternateBootDevice2, reboot, 01eh, 000h, 004h, 000h
CMOSName CMOS_AlternateBootDevice1, reboot, 01eh, 004h, 004h, 006h
CMOSName CMOS_PrimaryBootDevice4, critical, 01fh, 000h, 004h, 006h
CMOSName CMOS_PrimaryBootDevice3, critical, 01fh, 004h, 004h, 008h
CMOSName CMOS_PrimaryBootDevice2, critical, 020h, 000h, 004h, 000h
CMOSName CMOS_PrimaryBootDevice1, critical, 020h, 004h, 004h, 00ch
CMOSName CMOS_PS2Mouse, change, 02bh, 000h, 001h, 001h
CMOSName CMOS_FloppyRequired, reboot, 02bh, 006h, 001h, 000h
CMOSName CMOS_PostBootFailRequired, reboot, 02bh, 007h, 001h, 000h
CMOSName CMOS_iSCSIEnabled, change, 035h, 006h, 001h, 000h
CMOSName CMOS_SAS_ANNEX_ENABLE, change, 039h, 000h, 001h, 001h
CMOSName CMOS_StopOnError, reboot, 04ch, 000h, 002h, 001h
CMOSName CMOS_NV_NodeIntlv, change, 06ch, 005h, 001h, 000h
CMOSName CMOS_NV_ChipKill, change, 06dh, 004h, 001h, 001h
CMOSName CMOS_BMCPwrExec, change, 071h, 000h, 001h, 000h
CMOSName CMOS_ProcPerformanceStates, change, 071h, 001h, 001h, 000h
CMOSName CMOS_LowPowerHaltState, change, 071h, 002h, 001h, 000h
CMOSName CMOS_ENET2_PLANAR_ENABLE, change, 083h, 004h, 001h, 000h
CMOSName CMOS_ENET1_PLANAR_ENABLE, change, 083h, 003h, 001h, 000h
CMOSName CMOS_SAS_PLANAR_ENABLE, change, 083h, 007h, 001h, 000h
CMOSName CMOS_HPET_PLANAR_ENABLE, change, 084h, 004h, 001h, 001h
CMOSName CMOS_SerialA, change, 084h, 005h, 003h, 001h
CMOSName CMOS_SerialB, change, 085h, 000h, 003h, 000h
CMOSName CMOS_MMIOHoleRounding, change, 086h, 003h, 001h, 001h
CMOSName CMOS_PXE_NICSelect_Enable, reboot, 086h, 007h, 001h, 000h
CMOSName CMOS_UsbDisk, reboot, 0a0h, 000h, 001h, 001h
CMOSName CMOS_ENET_PXE_ENABLE, change, 0bch, 003h, 002h, 001h
CMOSName CMOS_NonPlanarPXE_Enable, change, 0bch, 005h, 001h, 000h
CMOSName CMOS_ReportUserDisabledPCIDevices, reboot, 0c8h, 003h, 001h, 000h
CMOSName CMOS_WakeOnLAN, reboot, 0cch, 004h, 001h, 001h
CMOSName CMOS_RemoteConsoleEnable, change, 0cch, 005h, 001h, 000h
CMOSName CMOS_RemoteConsoleEmulation, reboot, 0cch, 006h, 001h, 000h
CMOSName CMOS_RemoteConsoleKybdEmul, reboot, 0cch, 007h, 001h, 000h
CMOSName CMOS_RemoteConsoleComPort, reboot, 0ceh, 000h, 003h, 000h
CMOSName CMOS_RemoteConsoleBaud, reboot, 0ceh, 003h, 003h, 001h
CMOSName CMOS_RemoteConsoleDataBits, reboot, 0ceh, 006h, 003h, 003h
CMOSName CMOS_RemoteConsoleParity, reboot, 0cfh, 001h, 003h, 000h
CMOSName CMOS_RemoteConsoleStopBits, reboot, 0cfh, 004h, 003h, 000h
CMOSName CMOS_RemoteConsoleBootEnable, reboot, 0cfh, 007h, 001h, 000h
CMOSName CMOS_RemoteConsoleFlowCtrl, reboot, 0d0h, 000h, 001h, 000h
CMOSName CMOS_PCIBootPriority, change, 0d0h, 003h, 007h, 000h
CMOSName CMOS_ROMControlSlot1, reboot, 0BCh, 007h, 001h, 000h
CMOSName CMOS_ROMControlSlot2, reboot, 0BDh, 000h, 001h, 000h
CMOSName CMOS_ROMControlSlot3, reboot, 0BDh, 001h, 001h, 000h
CMOSName CMOS_ROMControlSlot4, reboot, 0BDh, 002h, 001h, 000h
CMOSName CMOS_ROMControlSlot5, reboot, 0BDh, 003h, 001h, 000h
CMOSName CMOS_ROMControlSlot6, reboot, 0BDh, 004h, 001h, 000h
CMOSName CMOS_ROMControlSlot7, reboot, 0BDh, 005h, 001h, 000h
CMOSChecksum 010h, 02dh, 02fh, 02eh
CMOSChecksum 07fh, 07fh, 03bh, 03ah
BMCSetting BMC_PrimaryBootDevice1, "First Primary Boot Device", critical, 184, 009:208.081.000.055.008.016|007#006, 010:208.081.000.055.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for First Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the first device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will be attempt to start from the",
                "second startup device."
        }
}
BMCSetting BMC_PrimaryBootDevice2, "Second Primary Boot Device", critical, 184, 009:208.081.000.056.008.016|007#006, 010:208.081.000.056.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for Second Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the second device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will be attempt to start from the",
                "third startup device."
        }
}
BMCSetting BMC_PrimaryBootDevice3, "Third Primary Boot Device", critical, 184, 009:208.081.000.057.008.016|007#006, 010:208.081.000.057.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for Third Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the third device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will be attempt to start from the",
                "fourth startup device."
        }
}
BMCSetting BMC_PrimaryBootDevice4, "Fourth Primary Boot Device", critical, 184, 009:208.081.000.058.008.016|007#006, 010:208.081.000.058.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for Fourth Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the fourth device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will halt with an error message."
        }
}

</pre></body></html>